
The new 5.8.0 version solves the following problems:
1. Add the "gap to model" configuration parameter to the brim of the hat
2. The hat brim supports judging whether to enable it based on the contact area between the model and the printing platform.
3. Add the function of wiping the mouth of the platform edge and spinning before pre-spinning.
4. Add model splitting function
5. Supports individually setting the filling density of small areas
6. Add the maximum traffic rate parameter
7. Other function optimization and bug modification